Ridge

Ring gear

High ground floor - floor

Basement- floor

-Thermo block 25cm; Thermal isolation; Facade lining

-Protection of waterproofing; Hydro isolation; AB wall 20cm

-trapezoidal metal sheets; 3cm laths; Batten 3cm; Vapor barrier; Osb; Batten; Thermal isolation; Foil; AB slab

-Flooring; Cement screed 5cm; Foil; Stirodur; AB slab 20cm

-Thermo block 25cm; Thermal insulation 10cm; Facade lining 12cm

- Molded floor; Cement screed 5cm; Stirodur 15cm; Betonitna ; AB slab 30cm; Gravel10cm

**Table 1**

Name - Architecture design

Name of drawing - Cross-section A-A