One potential tenderer requested following information:

**Clarification question:**

Please clarify the density of the plates signaling risks.

You mention 1000 x 700 x10 mm.

We had search for this density(10 mm) in the market and we have never found. The most appropriate density is 4 mm.

Please clarify if you accept this material or provide an alternative.

**Answer:**

According to the attribution documentation, dimensions for plates signaling risks are: 1000x700x10 mm (length, width, thickness); The density of the material from which they are made, is not specified.